CECInfo
(
	Name ( "pcie952_uart" )
	CECVersion ( 5.00 )
	GUID ( {0C12CB55-B70F-4C39-83BF-72051C1EA5E3} )
)
ComponentType
(
	Name ( "Uarts" )
	GUID ( {10861070-5F56-4AD5-A25D-C4F8B71F55AF} )
	Group ( "\device drivers\serial" )
	Vendor ( "oxsemi" )
	MaxResolvedImpsAllowed( 999 )
	Implementations
	(
		Implementation
		(
			Name ( "pcie952_uart" )
			GUID ( {ED145531-ACC3-4AD4-8267-3D05BBED09C1} )
			Version ( "1.0.0.0" )
			Locale ( 0409 )
			Vendor ( "oem" )
			Date ( "17/09/2007" )
			SizeIsCPUDependent( 1 )
			BuildMethods
			(
				BuildMethod
				(
					GUID ( {99983071-9A36-40E7-B1D4-27A285787891} )
					Step ( CESYSGEN )
					CPU ( "ARMV4I" )
					CPU ( "x86" )
					Action ( '#SRCCODE( USER_PROJECT, "$(_WINCEROOT)\OXSEMI\UARTS\pcie952_uart\pcie952_uart.pbpxml" )' )
				)
			)
		)
	)
)
